## Domanda 1

Considerando il processore MIPS64 e l’architettura descritta in seguito:

|  |  |  |
| --- | --- | --- |
| * + Integer ALU: 1 clock cycle   + Data memory: 1 clock cycle   + FP multiplier unit: pipelined 6 stages | * + FP divider unit: not pipelined unit that requires 6 clock cycles   + FP arithmetic unit: pipelined 4 stages   + branch delay slot: 1 clock cycle, and the branch delay slot disabled | * + forwarding enabled   + it is possible to complete instruction EXE stage in an out-of-order fashion. |

Usando il frammento di codice riportato, si calcoli il tempo di esecuzione dell’intero programma in colpi di clock e si completi la seguente tabella.

; for (i = 0; i < 100; i++) {

; v5[i] = (v1[i]+v2[i])\*(v3[i]+ v4[i]);

;}

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| .data |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | Clock  cycles |
| V1: .double “100 values” |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| V2: .double “100 values” |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| V3: .double “100 values”  …  V5: .double “100 zeros” |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| V4: .double “100 values” |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| V5: .double “100 values” |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| .text |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| main: daddui r1,r0,0 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| daddui r2,r0,100 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| loop: l.d f1,v1(r1) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| l.d f2,v2(r1) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| add.d f3,f1,f2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| l.d f1,v3(r1) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| l.d f2,v4(r1) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| add.d f4,f1,f2 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| mul.d f4,f4,f3 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| s.d f4,v4(r1) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| daddui r1,r1,8 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| daddi r2,r2,-1 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| bnez r2,loop |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| halt |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Total |  |  |  |  |  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |  |

**Domanda 2**

Considerando il programma precedente, e in particolare la coppia di istruzioni:

l.d f2,v2(r1)

add.d f3,f1,f2

che tipo di hazard crea l’utilizzo di f2 e come viene risolto? motivare la risposta.

**Domanda 3**

Considerando il programma precedente e l’architettura del processore superscalare descritto in seguito; completare la tabella relativa alle prime 3 iterazioni.

Processor architecture:

* + Issue 2 instructions per clock cycle
  + jump instructions require 1 issue
  + handle 2 instructions commit per clock cycle
  + timing facts for the following separate functional units:
    1. 1 Memory address 1 clock cycle
    2. 1 Integer ALU 1 clock cycle
    3. 1 Jump unit 1 clock cycle
    4. 1 FP multiplier unit, which is pipelined: 6 stages
    5. 1 FP divider unit, which is not pipelined: 7 clock cycles
    6. 1 FP Arithmetic unit, which is pipelined: 4 stages
  + Branch prediction is always correct
  + There are no cache misses
  + There are 2 CDB (Common Data Bus).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| # iteration |  | Issue | EXE | MEM | CDB x2 | COMMIT x2 |
| 1 | l.d f1,v1(r1) |  |  |  |  |  |
| 1 | l.d f2,v2(r1) |  |  |  |  |  |
| 1 | add.d f3,f1,f2 |  |  |  |  |  |
| 1 | l.d f1,v3(r1) |  |  |  |  |  |
| 1 | l.d f2,v4(r1) |  |  |  |  |  |
| 1 | add.d f4,f1,f2 |  |  |  |  |  |
| 1 | mul.d f4,f4,f3 |  |  |  |  |  |
| 1 | s.d f4,v4(r1) |  |  |  |  |  |
| 1 | daddui r1,r1,8 |  |  |  |  |  |
| 1 | daddi r2,r2,-1 |  |  |  |  |  |
| 1 | bnez r2,loop |  |  |  |  |  |
| 2 | l.d f1,v1(r1) |  |  |  |  |  |
| 2 | l.d f2,v2(r1) |  |  |  |  |  |
| 2 | add.d f3,f1,f2 |  |  |  |  |  |
| 2 | l.d f1,v3(r1) |  |  |  |  |  |
| 2 | l.d f2,v4(r1) |  |  |  |  |  |
| 2 | add.d f4,f1,f2 |  |  |  |  |  |
| 2 | mul.d f4,f4,f3 |  |  |  |  |  |
| 2 | s.d f4,v4(r1) |  |  |  |  |  |
| 2 | daddui r1,r1,8 |  |  |  |  |  |
| 2 | daddi r2,r2,-1 |  |  |  |  |  |
| 2 | bnez r2,loop |  |  |  |  |  |
| 3 | l.d f1,v1(r1) |  |  |  |  |  |
| 3 | l.d f2,v2(r1) |  |  |  |  |  |
| 3 | add.d f3,f1,f2 |  |  |  |  |  |
| 3 | l.d f1,v3(r1) |  |  |  |  |  |
| 3 | l.d f2,v4(r1) |  |  |  |  |  |
| 3 | add.d f4,f1,f2 |  |  |  |  |  |
| 3 | mul.d f4,f4,f3 |  |  |  |  |  |
| 3 | s.d f4,v4(r1) |  |  |  |  |  |
| 3 | daddui r1,r1,8 |  |  |  |  |  |
| 3 | daddi r2,r2,-1 |  |  |  |  |  |
| 3 | bnez r2,loop |  |  |  |  |  |

**Domanda 4**

Considerando il segmento di codice presentato nella tabella precedente, se assumiamo che il ROB ha una dimensione di 16 elementi e alla partenza del codice in tabella è vuoto, qual è la prima istruzione che dovrebbe stallare durante l’esecuzione del programma? motivare la risposta.